**Keypad:**

1-8 -> 0-8digital pins of Arduino

**Lcd(i2c convertor) to Arduino**

Gnd of i2c convertor to Gnd of arduino

Vcc of i2c convertor to 5V of arduino

Sda of i2c convertor to a4 of arduino

Scl of i2c convertor to a5 of arduino

**Gsm to Arduino**

Gnd of gsm to Gnd of arduino

Rx,Tx of gsm to 10,11 digital pins of arduino